50 GOTO 18900 100 X2=X/2000:Y2=Y/2000:N7=Y2:N8=(X-500)/1000 110 S5=X2-Z+Y2*Z:F4=X2<9 AND X2>0 AND Y2<9 AND Y2>0: RETURN 150 GOSUB 410:X=B9:Y=10: GOSUB 420 160 FOR I=1 TO K9: IF I>1 AND RND (900)>S(J) THEN 180 170 J= RND (64)+1: IF S(J) MOD 100>9 OR S(J)>800 THEN 170 180 S(J)=S(J)+100: NEXT I 185 FOR I=1 TO 64:Q(I)=-S(I)-2- RND (4)- RND (4): NEXT I 190 Q3= RND (64)+1:S3= RND (64)+1:Q(Q3)=-Q(Q3): GOSUB 600: GOTO 3200 200 Q(Q3)= ABS (Q(Q3)): GOSUB 410:N=Q(Q3):S4=N MOD 10:K=N/100:B=N/10-K*10 210 S(S3)=1:X=B:Y=2: GOSUB 420:X=S4:Y=3: GOSUB 420:X=K:Y=-S9: GOSUB 420 230 S6=S3: RETURN 300 NA= PEEK (34): POKE 34,11: INPUT "COURSE",C: POKE 34,NA 305 C= ABS (C) MOD 360:C1=C/90:C2=C MOD 90 310 IF C1 MOD 2=0 THEN 330:C2=90-C2 330 GOSUB 370:X1=C3:C2=90-C2: GOSUB 370:Y1=C3 340 IF C1 MOD 3=0 THEN Y1=-Y1: IF C1>1 THEN X1=-X1: RETURN 370 C3=167*C2-26*(C2-30)*(C2>30)-38*(C2-45)*(C2>45)-58*(C2-60)*(C2>60) 375 C3=(C3+5)/10: RETURN 410 FOR I=1 TO 64:S(I)=0: NEXT I: RETURN 420 IF X=0 THEN RETURN : FOR I=1 TO X 430 J= RND (64)+1: IF S(J)#0 THEN 430:S(J)=Y: NEXT I: RETURN 450 GOSUB 480:X=S1-J1:Y=S2-J2 460 X1=X*X+Y*Y: IF X1>9 THEN H=(9*H)/X1 470 PRINT H;" UNIT HIT ON";: RETURN 480 J1=1+(J-1)/8:J2=1+(J-1) MOD 8 490 S1=1+(S3-1)/8:S2=1+(S3-1) MOD 8 495 Q1=1+(Q3-1)/8:Q2=1+(Q3-1) MOD 8: RETURN 500 IF K=0 THEN RETURN : IF NOT N6 THEN N4=0: GOSUB 630 505 S7=1+(S6-1)/8:S8=1+(S6-1) MOD 8 510 FOR J=1 TO 64:J4=J: IF S(J)<0 THEN 520: NEXT J:S6=S3: RETURN 520 GOSUB 480:C5=S7-J1:C6=S8-J2: GOSUB 2030: IF S(J) MOD 100=0 OR ( ABS (C5)+ ABS (C6))< RND (5) THEN 575 530 GOSUB 1520: IF V3=0 THEN 570 540 T$="#":P1=0:W=R: GOSUB 1200: IF S(S5)#0 AND S(S5)#1 THEN 570 550 PRINT " < ";: GOSUB 1450: PRINT " FIRING ";D$(41,47);" >" 560 PRINT : GOSUB 2400:J=J4: GOSUB 2030:V3=V3-1: GOTO 580 570 IF R+ RND (3)<6 THEN 575: NEXT J:S6=S3: RETURN 575 GOSUB 1105:N1=S1:N2=2*S2: GOSUB 1175: GOSUB 1420:H=(V1* RND (10))/20:V1=V1-H 577 GOSUB 450: PRINT A$;"FROM": GOSUB 1450: PRINT : GOSUB 817:J=J4 580 GOSUB 2050: GOSUB 1100: NEXT J:S6=S3: RETURN 600 POKE 34,0: POKE 35,24: GOSUB 640: CALL -936: RETURN 610 POKE 32,18: POKE 33,23 620 POKE 34,13: POKE 35,24: CALL -936: RETURN 630 POKE 34,N4: POKE 35,13 640 POKE 32,0: POKE 33,40: VTAB 13: TAB 1: RETURN 660 N4=0: GOSUB 630: CALL -936: RETURN 670 POKE 32,0: POKE 33,40: VTAB Q1: TAB (4*Q2+1): PRINT " ";: TAB (4*Q2+1): PRINT Q(Q3): GOTO 630 680 POKE 32,1: POKE 33,16: GOSUB 620: VTAB 14: RETURN 690 CALL -384: GOSUB 670: CALL -380: RETURN 695 GOSUB 690: IF Q(Q7)<0 THEN RETURN : TAB (4*Q6+1): VTAB Q5: PRINT Q(Q7): GOTO 630 800 E=E0:P=P0:E1=(E/100)*E2: FOR D1=1 TO 9:D(D1)=0: NEXT D1: RETURN 815 GOSUB 7020:H=200+ RND (400): PRINT "SPACE STORM!!": GOSUB 1420: GOSUB 470: PRINT A$: GOSUB 490 817 E=E-H:E1=E1-H: IF E1<0 THEN E1=0: GOSUB 1030: IF H<10 THEN RETURN : IF E1>= RND (H/10)* RND (20) THEN RETURN 820 GOSUB 1030:E1=5:D1= RND (8+(D(9)=0))+1: IF D1=6 THEN 840:D(D1)=D(D1)+5+ RND (30): IF D1=9 THEN 845 825 IF D1=2 THEN GOSUB 1000 830 GOSUB 1440: PRINT A$;" DAMAGED ";D(D1)/100;".";D(D1) MOD 100;" YRS TO REPAIR" 835 IF D1=7 THEN 843: RETURN 840 GOSUB 1440: GOSUB 1470:D(6)=0: FOR I=1 TO 64:Q(I)=- ABS (Q(I)): NEXT I:Q(Q3)=-Q(Q3): IF NOT N6 THEN RETURN :N6=0: GOTO 3200 843 A1=0:A2=4: GOSUB 1620:A2=5: GOSUB 1620: RETURN 845 PRINT "DILITHIUM CRYSTALS DESTROYED!": RETURN 850 IF D(9)=0 THEN E=E+50*T3:E3=E0+5000-P*500: IF E>E3 THEN E=E3: FOR T2=1 TO T3 852 E3=((E/10)*(E2/10)+(E/100)*E2 MOD 10-E1)/4:E1=E1+E3: NEXT T2 860 T1=T1+T3:T=T+T1/100:T1=T1 MOD 100: GOSUB 1030: IF RND (150)0 AND D(D1)-T3<1 THEN GOSUB 990 890 IF D(D1)>0 THEN D(D1)=D(D1)-T3: NEXT D1 900 D1= RND (Z)+1: IF RND (100)>25 OR D(D1)=0 THEN RETURN 910 PRINT "** SPOCK USED A NEW REPAIR TECHNIQUE **" 990 D(D1)=0: GOSUB 1440: PRINT A$;" REPAIRED!": IF D1=2 THEN 1000: IF D1=3 AND N6 THEN GOSUB 3205: RETURN 1000 IF N6 THEN GOSUB 3205: GOSUB 680: PRINT " QUADRANT ";Q1;"-";Q2: IF D(2) THEN 1010: FOR I=1 TO 64:G=S(I)+2: IF G<2 THEN G=1 1005 D$(2*I-1)=Q$(G,G):D$(2*I)=" ": NEXT I: CALL -384: PRINT D$: GOTO 1020 1010 GOSUB 490: POKE 32,0: FOR N1=S1-1 TO S1+1: FOR N2=2*(S2-1) TO 2*(S2+1): GOSUB 1120: NEXT N2: NEXT N1: POKE 32,1 1020 CALL -384: VTAB 23: TAB 1: PRINT "1 2 3 4 5 6 7 8";: VTAB 15: POKE 32,16: POKE 33,1 1025 CALL -380: PRINT "12345678";: GOSUB 630 1030 GOSUB 610:N5=0: PRINT "SECTOR","",S1;"-";: CALL -384: PRINT S2: CALL -380 1035 IF T1=0 THEN 1040:T2=T9-T-1:T4=100-T1: GOTO 1045 1040 T2=T9-T:T4=0 1045 PRINT "YEARS","",T2;".";T4: PRINT "STARDATE",T;".";T1/10 1047 A$="GREEN": IF E1<(E0/10) OR E-E1<(E0/10) THEN A$="YELLOW": IF K THEN A$="RED" 1050 IF A$#"GREEN" THEN POKE 50,127: PRINT "CONDITION",A$: CALL -380: PRINT "SHIELDS ",E2;"%": GOSUB 1430: PRINT A$,E1 1060 GOSUB 1400: PRINT "AVAIL ENERGY",E-E1: PRINT D$(41,50),P 1070 PRINT "KLINGONS",K9: PRINT "BASES","",B9 1075 PRINT "COURSE ";: IF A1=0 THEN PRINT "NOT SET."; 1080 IF NOT A1 THEN 630: PRINT "SET FOR ";V5;"-";: CALL -384: PRINT V6;: CALL -380: GOTO 630 1100 N1=J1:N2=2*J2: GOTO 1120 1102 N1=S1:N2=2*S2: GOTO 1120 1105 N1=J1:N2=2*J2: GOTO 1125 1107 N1=S1:N2=2*S2: GOTO 1125 1110 GOSUB 1180 1115 IF T$#"E" THEN CALL R5-95 1116 CALL -384: VTAB (N1+14): TAB N2: PRINT T$;: GOTO 1145 1120 CALL -384 1125 GOSUB 1180: VTAB (N1+14): TAB N2 1130 G=2: IF N2 MOD 2 THEN 1140 1135 N3=N2/2-Z+Z*N1:G=S(N3)+2: IF G<2 THEN G=1 1140 PRINT Q$(G,G); 1145 CALL -380: VTAB 13: TAB 1: RETURN 1170 T$="#": POKE R5-94,6: POKE R5-80,200: GOSUB 1110: GOTO 1120 1175 T$="#": POKE R5-94,7: POKE R5-80,140: GOSUB 1110: GOTO 1120 1180 IF N2<2 OR N2>16 OR N1<1 OR N1>8 THEN 1190: IF NOT D(2) THEN RETURN : IF ABS (N1-S1)<2 AND ABS (N2-2*S2)<3 THEN RETURN 1190 CALL -380: POP : RETURN 1200 POKE R5-94,1: POKE R5-80,180: GOSUB 480:F1=0 1202 IF T$="E" THEN S(S3)=0 1205 N1=J1:N2=2*J2:X=2000*J2+1000:Y=2000*J1+1000 1210 FOR I=1 TO 2*W:F2=(I+1)/2 1220 X=X+X1:Y=Y+Y1: GOSUB 100: IF N1=N7 AND N2=N8 THEN 1250 1225 IF P1 THEN GOSUB 1120:N1=N7:N2=N8: IF NOT F4 THEN 1290: IF P1 THEN GOSUB 1110 1230 IF X2=J2 AND Y2=J1 THEN 1250: IF S(S5)#0 THEN 1252 1250 NEXT I: IF P1 THEN 1120: RETURN 1252 IF S(S5)<0 THEN GOSUB 1410: IF S(S5)=1 THEN GOSUB 1420: IF S(S5)=2 THEN 1280: IF S(S5)=3 THEN A$="STAR" 1260 F1=2:I=W*2: NEXT I:W=F2: GOTO 1120 1280 GOSUB 800:S(S5)=0:B9=B9-1: PRINT "":Q(Q3)=Q(Q3)-10: GOSUB 1030: IF N6 THEN GOSUB 690: GOTO 1250 1290 F1=1:I=2*W: NEXT I:W=W-F2: RETURN 1320 Q5=Q1+(Y2>8)-(Y2<1):Q6=Q2+(X2>8)-(X2<1) 1330 Q5=(Q5+7) MOD Z+1:Q6=(Q6+7) MOD Z+1 1340 Q7=Q6-Z+Z*Q5: RETURN 1350 Y2=(Y2+15) MOD Z+1:X2=(X2+15) MOD Z+1: GOTO 110 1400 D$="WARP DRIVESR SENSORSLR SENSORSPHASERS PH TORPS GAL RECORDCOMPUTER PROBE ": RETURN 1410 A$=" KLINGON ": RETURN 1420 A$=" ENTERPRISE ": RETURN 1430 A$="SHIELD ENERGY ": RETURN 1440 GOSUB 1400:A$=D$(10*D1-9,10*D1): RETURN 1450 GOSUB 1410: PRINT A$;"AT "; 1455 PRINT J1;"-";: CALL -384: PRINT J2;: CALL -380: PRINT " ";: RETURN 1460 PRINT "( ";V1;" LEFT )": RETURN 1470 PRINT A$;" DESTROYED!!!": RETURN 1510 IF ABS (C5)>4 THEN C5=C5-Z* SGN (C5): IF ABS (C6)>4 THEN C6=C6-Z* SGN (C6) 1520 C= PEEK ( ABS (C5)+Z*( ABS (C6))+R5-65) 1530 IF C5<0 THEN C=180-C 1540 IF C6<0 THEN C=360-C 1550 GOSUB 305:X=1000* SGN (X1):Y=1000* SGN (Y1) 1560 FOR I=1 TO 30:X=X+X1:Y=Y+Y1:R=I/2: IF I MOD 2 THEN 1580 1570 IF Y/2000#C5 OR X/2000#C6 THEN 1580:I=30 1580 NEXT I: RETURN 1600 VTAB 13: TAB 1: CALL -868: PRINT "COORDINATE ?-";: CALL -384: PRINT " ";: CALL -380 1605 GOSUB 2510: IF KB<1 OR KB>8 THEN 1605: TAB 12: PRINT KB;:Y2=KB: CALL -384: TAB 14: PRINT "?"; 1610 GOSUB 2510: IF KB<1 OR KB>8 THEN 1610:X2=KB: TAB 14: PRINT KB;: CALL -380: TAB 1: CALL -868: RETURN 1620 FOR I=1 TO 64: IF 3-A2=S(I)/10000 THEN S(I)=S(I) MOD 10000: NEXT I: RETURN 1640 PRINT :D1=A2: GOSUB 1440 1650 B1=0: FOR J=1 TO 64: IF S(J)/10000=(3-A2) THEN 1660: NEXT J: GOTO 1680 1660 B1=B1+1: GOSUB 480: IF B1=1 THEN PRINT A$;" LOCKED ON ": GOSUB 1455: NEXT J 1680 IF B1=0 THEN PRINT A$;" NOT LOCKED";: PRINT : RETURN 1685 A2=4: GOSUB 1640:A2=5: GOTO 1640 1800 IF K=0 THEN RETURN :K4= NOT K4 1810 FOR J=1 TO 64: IF S(J) MOD 1000>-40 OR S(J) MOD 2#-K4 THEN 1900 1840 GOSUB 2030: GOSUB 480:C5=J1-S1:C6=J2-S2 1845 IF (V1> RND (400))-(K=1)+(K>3) THEN 1850:C5=-C5:C6=-C6 1850 Y2=J1-(C5>0)* RND (2):X2=J2-(C6>0)* RND (2): GOSUB 110 1860 IF F4=1 THEN 1880: IF V1> RND (400) OR (K<4 AND RND (5)#0) THEN 1900 1870 GOSUB 1320:K=K-1:S(J)=0:Q(Q3)=Q(Q3)-100:Q(Q7)=Q(Q7)+100* SGN (Q(Q7)): GOSUB 1100 1875 IF N6 THEN GOSUB 695: NEXT J: RETURN 1880 IF S(S5)#0 THEN 1900 1890 V1=V1-20: GOSUB 2050:S(S5)=S(J):S(J)=0:N1=J1:N2=2*J2: GOSUB 1120:N1=Y2:N2=2*X2: GOSUB 1120 1900 NEXT J: RETURN 2030 V1=-S(J) MOD 1000:V2=-S(J)/10000:V3=-(S(J)/1000) MOD 10: RETURN 2050 IF V1<=0 THEN 2060: IF V1<20 THEN V3=0:S(J)=-V1-1000*V3-10000*V2:S(J)=S(J)+(S(J) MOD 2=-K4): RETURN 2060 GOSUB 1410: GOSUB 1470:S(J)=0:K=K-1:K9=K9-1:Q(Q3)=Q(Q3)-100: GOSUB 1100 2065 N1=Y2:N2=2*X2: GOSUB 1120: IF N6 THEN GOSUB 690: GOTO 1030 2200 T3=1: GOSUB 850: IF A1=0 THEN RETURN 2210 C5=V5-S1:C6=V6-S2: IF C5=0 AND C6=0 THEN 2240: GOSUB 1520 2220 W=1: GOSUB 5267: GOSUB 490:E=E-30: GOSUB 1030: IF V5#S1 OR V6#S2 THEN RETURN 2240 A1=0: RETURN 2400 W=15:P1=1:T$="#": GOSUB 1200: IF F1=2 THEN 2420: PRINT "MISSED!!": RETURN 2420 N1=Y2:N2=2*X2: GOSUB 1170: PRINT D$(41,47);" HIT ON ";A$;" AT ";Y2;"-";: CALL -384: PRINT X2: CALL -380 2430 IF S(S5)=2 THEN RETURN : IF S(S5)>0 THEN 2460:J=S5: GOSUB 2030:V1=V1-500: GOSUB 1460: GOTO 2050 2460 IF S(S5)#1 THEN 2470:H=500: GOTO 817 2470 GOSUB 1470:Q(Q3)=Q(Q3)-1:S(S5)=0:N1=Y2:N2=2*X2: IF N6 THEN GOSUB 690: GOTO 1120 2500 KB= PEEK (-16384): IF KB<128 THEN 2500: POKE -16368,0: RETURN 2510 GOSUB 2500: IF KB<176 OR KB>185 THEN KB=-1:KB=KB MOD 16: RETURN 3200 IF N6 THEN RETURN : GOSUB 490 3202 GOSUB 660:N6=1: FOR Q6=1 TO Z: TAB 4: PRINT ": : : : : : : : :": NEXT Q6:N4=9: GOSUB 630: GOSUB 690 3205 X=Q7: IF D(3) THEN 3220 3210 FOR I=-1 TO 1: FOR Y=-1 TO 1:Q5=Q1+I:Q6=Q2+Y: GOSUB 1330:Q(Q7)= ABS (Q(Q7)): NEXT Y,I 3220 FOR Q7=1 TO 64: IF Q(Q7)<0 THEN 3230:I=1+(Q7-1)/8:Y=1+(Q7-1) MOD 8: TAB (4*Y+1): VTAB I 3225 PRINT " ";: TAB (4*Y+1): PRINT Q(Q7);: IF Q7=Q3 THEN GOSUB 690 3230 NEXT Q7:Q7=X: GOTO 630 5200 A1=0: GOSUB 3200: IF NOT D(1) THEN 5220: PRINT "ION DRIVE ONLY": GOTO 5250 5220 PRINT "WARP OR ION DRIVE (W OR I)?";: GOSUB 2500: TAB 1: CALL -868: IF KB=201 THEN 5250: IF KB#215 THEN RETURN 5240 PRINT "WARP FACTOR(1-6)?";: GOSUB 2510:W=KB: TAB 1: CALL -868: IF W<1 OR W>6 THEN RETURN : IF E-E1>=12*W ^ 3 THEN 5360: PRINT "NOT ENOUGH ENERGY": GOTO 5240 5250 PRINT "DURATION(1-9)?";: GOSUB 2510: TAB 1: CALL -868:W=KB: IF W<1 THEN RETURN : IF E-E1>=20*(1+W) THEN 5260: PRINT "NOT ENOUGH ENERGY": GOTO 5250 5260 GOSUB 300 5265 GOSUB 1800 5267 W1=0 5270 IF W=0 THEN 5340:P1=1:T$="E":J=S3: GOSUB 1200 5280 W1=W1+F2: IF F1=0 THEN 5340 5290 IF F1=1 THEN 5350: IF S(S5)=1 THEN 5270 5320 PRINT "STOPPED BY ";A$;" AT ";Y2;"-";: CALL -384: PRINT X2: CALL -380 5330 X=X-X1:Y=Y-Y1: GOSUB 100 5340 S(S3)=0:S(S5)=1:S3=S5: GOSUB 1102: GOSUB 490: GOSUB 1102 5342 IF D(2) THEN GOSUB 1000: IF A1 THEN RETURN 5345 E=E-20*(1+W1):T3=W1: GOSUB 850: GOTO 500 5350 GOSUB 1320: GOSUB 670:Q3=Q7: GOSUB 1350:S3=S5: GOSUB 490: GOSUB 200: GOSUB 1000: GOTO 5270 5360 GOSUB 300: GOSUB 490 5365 Q5=Q1+((W*Y1)+500*( SGN (Y1)))/1000:Q6=Q2+((W*X1)+500*( SGN (X1)))/1000 5367 GOSUB 1330:Q9=Q7:Q7=Q3:W9=W:A1=1:W=3: GOSUB 5265:A1=0: IF F1=2 THEN 5340 5368 IF Q7#Q9 THEN GOSUB 670:Q3=Q9:W=W9: IF Q7=Q9 THEN 5380:S3= RND (64)+1 5375 GOSUB 200: GOSUB 490: GOSUB 1000 5380 E=E-12*W ^ 3:T3=10: GOSUB 850: GOTO 500 5400 GOSUB 1430: PRINT "SET ";A$;"%";: INPUT E2: GOTO 1030 5600 GOSUB 660:N6=0: FOR D1=1 TO Z: IF D1=6 THEN NEXT D1: IF D(D1)>0 THEN 5605: GOSUB 1440: PRINT A$,"OK": GOTO 5610 5605 GOSUB 830 5610 NEXT D1:N4=8: IF D(9)<=0 THEN 630: GOSUB 845:N4=9: GOTO 630 5800 IF NOT D(4) THEN 5805:D1=A: GOTO 830 5805 IF NOT N6 THEN N4=0:A2=A: GOSUB 1640: GOSUB 6140: IF IB#193 AND B1 THEN RETURN : IF A=4 THEN 5830 5810 IF P>=B1 AND P#0 THEN 5820: PRINT "EXCUSE ME SIR, WE HAVE ";P;" LEFT.": PRINT : RETURN 5820 IF B1>0 THEN 5850: INPUT "TRAJECTORY",C9: IF C9>359 THEN RETURN : GOTO 5850 5830 PRINT : INPUT "PHASERS READY: ENERGY TO FIRE",H1: IF H1<1 THEN RETURN 5840 IF H1<=E-E1 THEN 5850: PRINT "EXCUSE ME SIR, WE ONLY HAVE ";E-E1;".": GOTO 5830 5850 IF K=0 AND A=4 THEN RETURN :K7=K: IF B1=0 THEN 5867 5860 K7=B1: GOSUB 1800: GOSUB 2200: GOSUB 500:A2=A: GOSUB 1640 5865 IF D(A)>0 OR B1=0 THEN RETURN 5867 IF A=5 THEN 6080 5870 IF H1>E-E1 THEN H1=E-E1: FOR J=1 TO 64: IF S(J)>=0 THEN 5895: GOSUB 2030: IF V2#1 AND B1>0 THEN 5895 5875 GOSUB 480: GOSUB 1107 5880 N1=J1:N2=2*J2: GOSUB 1175:H=H1/K7:E=E-H: GOSUB 2030: GOSUB 450:V1=V1-H 5890 GOSUB 1450: PRINT : GOSUB 1460: GOSUB 2050: GOSUB 1102: NEXT J: GOTO 6100 5895 NEXT J: GOTO 6100 6000 IF NOT D(5) THEN 5805:D1=A: GOTO 830 6080 IF B1#0 THEN 6090:C=C9: GOSUB 6130: GOTO 6100 6090 FOR J=1 TO 64: IF S(J)/10000=-2 THEN GOSUB 6120: NEXT J 6100 GOSUB 1030: IF B1#0 THEN RETURN : GOSUB 1800: GOSUB 2200: GOTO 500 6120 GOSUB 480:C5=J1-S1:C6=J2-S2: GOSUB 1520 6130 GOSUB 305: GOSUB 1420: PRINT " < ";A$;"FIRING ";D$(41,47);" >":J9=J:J=S3: GOSUB 2400:J=J9:P=P-1: RETURN 6140 IF B1=0 THEN RETURN : PRINT "AUTO OR MANUAL (A OR M)?";: GOSUB 2500: TAB 1: CALL -868:IB=KB: IF IB=205 THEN B1=0: RETURN 6200 INPUT "# TO LOAD (+) OR UNLOAD (-)",N: IF N<-P OR N>10-P THEN 1030:E=E-(500+100* SGN (N))*N:P=P+N: GOTO 1030 6400 IF NOT D(7) THEN 6402:D1=7: GOTO 830 6402 E=E-20: GOSUB 640 6405 PRINT : PRINT "APPLE-81 HERE-" 6410 N5=1: GOSUB 610: PRINT "1 *COMPUTE QUADRANT": PRINT "2 *LOCK PHASERS": PRINT "3 *LOCK PH TORPS" 6430 PRINT "4 *LOCK COURSE": PRINT "5 *COMPUTE TRAJECTORY": PRINT "6 *RETURN": GOSUB 630 6440 PRINT "WHAT IS YOUR INSTRUCTION?";: GOSUB 2510:B=KB: TAB 1: CALL -868: IF B<1 OR B>6 THEN 6410: IF N5 THEN GOSUB 1030: IF B>1 THEN 6530 6460 GOSUB 1600:C5=Y2-Q1:C6=X2-Q2: GOSUB 1510: GOSUB 6695: PRINT "COURSE - ";C,"WARP - ";R: GOSUB 630: GOTO 6440 6530 IF B>3 THEN GOTO 6610+10*B 6540 A2=B+2: GOSUB 1620 6550 PRINT "# OF TARGETS?";: GOSUB 2510: TAB 1: CALL -868:B1=KB: IF B1=0 THEN 6440: IF B10 THEN 6570: GOSUB 6690: GOTO 6640 6570 FOR I=1 TO B1: GOSUB 1600: GOSUB 1350: IF S(S5)<0 THEN 6620: GOSUB 6690: GOTO 6630 6620 J=S5: GOSUB 2030:V2=B-1: GOSUB 2050 6630 NEXT I 6640 E=E-20: GOTO 6440 6650 A1=1: GOSUB 1600:V5=Y2:V6=X2: GOSUB 1030: GOTO 6640 6660 GOSUB 1600:C5=Y2-S1:C6=X2-S2: GOSUB 1520: GOSUB 6695: PRINT "TRAJECTORY - ";C,"RANGE - ";R: GOSUB 630: GOTO 6440 6670 CALL -936: RETURN 6690 CALL -384: PRINT "";: CALL -380: TAB 1: RETURN 6691 CALL -936: VTAB 13: PRINT "APPLE-81 HERE-": RETURN 6695 IF N4=0 THEN N4=1: POKE 34,N4-1: VTAB N4: TAB 1: CALL -868: RETURN 6800 IF NOT D(8) THEN 6805:D1=8: GOTO 830 6805 E=E-30: GOSUB 1030: PRINT : IF K#0 THEN 6810: TAB 10: PRINT "> NO KLINGONS <": RETURN 6810 GOSUB 660: CALL -384: PRINT "COORD","ENERGY","TORPS","LOCK": CALL -380 6820 FOR J=1 TO 64: IF S(J)<0 THEN 6830: GOTO 6860 6830 GOSUB 480: GOSUB 2030: TAB 2: PRINT J1;"-";: CALL -384: PRINT J2;: CALL -380: PRINT " ",V1,V3; 6840 IF V2 THEN 6850: PRINT : GOTO 6860 6850 D1=V2+3: GOSUB 1440: TAB 24: PRINT A$ 6860 NEXT J:N4=K+2:N6=0: GOTO 630 7000 GOSUB 9800: INPUT SD1$: IF SD$#SD1$ THEN RETURN 7005 FOR I=1 TO 4: GOSUB 7020: NEXT I 7010 A=4:A2=4:H1=E+500*P+1000: GOSUB 1620:K7=K:B1=-1: GOSUB 5870:E=0:P=0: POP : GOTO 9400 7020 POKE R5-89,105: POKE R5-94,1: POKE R5-80,255 7030 POKE -16304,0: POKE -16302,0: CALL R5-95 7040 POKE -16303,0: FOR J=1 TO 50: NEXT J: POKE R5-89,233: RETURN 9005 TEXT :J=I=S3=S5: DIM S(64),Q$(5),D$(128),Q(64):Q$="K EB*" 9010 Z=8:X=Y=X2=Y2=K4=V1=V2=V3: DIM I$(8),D(9),A$(14) 9015 DIM SD$(10),SD1$(10) 9020 R5=16384 9030 GOSUB 600:N6=0 9051 VTAB 9: TAB 12: PRINT ",";: TAB 28: PRINT "," 9052 TAB 12: CALL -384: PRINT "A";: CALL -380: PRINT " APPLE II TREK ";: CALL -384: PRINT "A": CALL -380: VTAB 16 9055 B9=2+ RND (2)+ RND (2):K9=25+ RND (15)+ RND (15) 9060 S9=3800:T9=3427:T0=3424:T=T0:E0=5000:P0=10:T1=0:E2=50 9065 A1=0: GOSUB 800:K0=K9:B0=B9 9070 PRINT "CAPTAIN'S LOG - STARDATE ";T0;".";T1: PRINT 9075 PRINT "WE HAVE BEEN ASSIGNED A ";T9-T0;" YEAR MISSION" 9080 GOSUB 1410: PRINT "TO SEEK AND DESTROY ";K9;A$;"BATTLE" 9085 PRINT "CRUISERS. WE WILL HAVE ";B9;" BASES AVAILABLE" 9090 IF IB=217 THEN 9200: POKE R5-89,233: PRINT "DIFFERENT SET-UP?";: GOSUB 2500: TAB 1: CALL -868 9110 IF KB#217 THEN 9200: POKE 34,12: CALL -936: VTAB 23 9120 PRINT "SET UP YOUR OWN?";: GOSUB 2500: TAB 1: CALL -868:IB=KB: IF IB#217 THEN 9055 9135 INPUT "KLINGONS(200 MAX)",K9: IF K9>200 OR K9<1 THEN 9135 9140 INPUT "BASES(20 MAX)",B9: IF B9>20 OR B9<1 THEN 9140: GOTO 9065 9200 GOSUB 9800: INPUT SD$: GOSUB 150: GOSUB 200: GOSUB 1000: GOSUB 500 9220 GOSUB 490: GOSUB 630:N5=0 9225 POKE R5-80,3: POKE R5-94,50: CALL R5-95: PRINT " COMMAND?";: GOSUB 2510:A=KB: TAB 1: CALL -936: VTAB 13 9230 IF N5 THEN GOSUB 1030: IF A>0 AND A<10 THEN 9310:N5=1: GOSUB 610 9245 PRINT "1 NAVIGATION": GOSUB 1430: PRINT "2 ";A$ 9250 PRINT "3 DAMAGE RPT": PRINT "4 ";D$(31,40): PRINT "5 ";D$(41,50): PRINT "6 LOAD ";D$(41,50) 9260 PRINT "7 ";D$(61,70): PRINT "8 ";D$(71,80): PRINT "9 SELF-DESTRUCT" 9275 GOSUB 630: GOTO 9225 9310 GOSUB 5000+A*200+(A>7)*200 9320 IF K9>0 AND E>0 AND E>E1 AND T9>T THEN 9220 9400 X1=(K0-K9)*100:Y1=(B0-B9)*50+E/200: IF NOT Y1 THEN Y1=1:X=2*(X1/Y1+X1/((T-T0)*100+1+T1))-K9-4*B0 9405 GOSUB 600: VTAB 3: TAB 12: PRINT "< BULLETIN >": PRINT 9410 PRINT "STARDATE ";T;".";T1/10: PRINT : PRINT "TO: ALL UNITS": PRINT "FROM: STARFLEET COMMAND": PRINT 9420 D$="SUCCESSFUL": IF K9 THEN D$="UNSUCCESSFUL": IF E<=0 OR E<=E1 THEN D$="DESTROYED": GOSUB 1420 9430 PRINT "WE HAVE BEEN NOTIFIED THAT THE STARSHIP": PRINT A$;"HAS BEEN ";D$;" AFTER" 9440 D$="ALL ": IF K9 THEN D$="ONLY " 9450 PRINT T-T0;".";T1/10;" YEARS OF ITS ";T9-T0;" YEAR MISSION. THE": PRINT A$;"DESTROYED ";D$;K0-K9;: GOSUB 1410: PRINT A$ 9470 PRINT "BATTLE CRUISERS";: IF K9 THEN PRINT " OF ";K0;: PRINT " IN ITS MISSION.": PRINT 9480 D$="DISASTROUS": IF X>30 THEN D$="LACKLUSTER": IF K9 THEN 9490:D$="EXCELLENT": IF X>60 THEN D$="BRILLIANT" 9490 PRINT "THIS ";D$;" PERFORMANCE MEANS" 9500 IF K9 AND X<30 THEN 9520: IF K9 THEN 9530 9510 PRINT "VICTORY FOR";: GOTO 9540 9520 PRINT "DESTRUCTION OF";: GOTO 9540 9530 PRINT "DIFFICULT TIMES FOR"; 9540 PRINT " THE FEDERATION.": PRINT 9550 PRINT "STARFLEET COMMAND HEREBY ISSUES ORDERS": PRINT "FOR "; 9555 IF K9 AND X<30 THEN 9570: IF K9 THEN 9580: IF X>60 THEN 9590 9560 PRINT "THE MEDAL OF VALOR";: GOTO 9600 9570 PRINT "DISMISSAL FOR INCOMPETENCE";: GOTO 9600 9580 PRINT "REMOVAL FROM COMMAND";: GOTO 9600 9590 PRINT "PROMOTION TO ADMIRAL"; 9600 PRINT " FOR THE": GOSUB 1420: PRINT "CAPTAIN OF THE";A$;"FOR A" 9610 PRINT "BATTLE FACTOR OF ";X;" IN THIS MISSION." 9700 IB=0: PRINT : PRINT "TRY AGAIN?";: GOSUB 2500: PRINT : IF KB=217 THEN 9030 9710 END 9800 PRINT : PRINT "ENTER SELF-DESTRUCT PASSW0RD-";: RETURN 10000 REM W SANDER 1/11/78 18900 HIMEM:16384 19000 GOTO 9005 19900 REM HIMEM:41479 HIMEM:59672 36348 SGN @h` PrPm IF k IF A 20000 REM 44444444,4162543945300423931442146, VLIN DSP 3828723197,, IN#3751725946= NODSP 3597525434 VLIN , DSP 35719, PRINT ,= NODSP PR#391M 44444444,4162543945300423931442146, VLIN DSP 3828723197,, IN#3751725946= NODSP 3597525434 VLIN , DSP 35719, PRINT ,= NODSP P HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM:0 HIMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:IMEM:I HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM: HIMEM:<= DEL <>,<> AUTO <> CLR <> NEW <>,<> DEL <> RUN <> RUN <> CON <> SAVE <> LOAD <>:<> _ <>