`SPEZIFICATION

| `MICROPROCESSOR:` |  | `MOS TECHNOLOGY 6502`
| `Micorprocessor Clock Frequency:` |  | `1.023 MHz`
| `Effective Cycle Frequency: (Including Refresh Waits)` |  | `0.960 MHz`
| `VIDEO OUTPUT` |  | `Composite positive video, 74 ohms, level adjustable between zero and +5Vpp.`
| `Line Rate:` |  | `15734 Hz`
| `Frame Rate:` |  | `60.05 Hz`
| `Format:` |  | `40 characters/line, 24 lines; with automatic scrolling`
| `Display Memory:` |  | `Dynamik shift registers (1K x 7)`
| `Character Matrix:` |  | `5 x 7`
| `RAM MEMORY:` |  | `16-pin, 4K Dynamic, type 4096 (2104)`
| `On-board RAM Capacity:` |  | `8K bytes (4K supplied)`
| `POWER SUPPLIES:` |  | `+5 Volts @ 3 amps, +/.12 Volts @ 0.5 amps, and -5 Volts @ 0.5 amps`
| `Input Power Requirements:` |  | `8 to 10 Volts AC (RMS) @ 3 amps, 26 to 28 Volts AC (RMS) Center-Tapped, 1A.`
| `Recommended Transformers:` |  | `Stancor # P-8380 or Triad F31-X Stancor # P-8667 or Triad F40-X`

| APPLE COMPUTER COMPANY 770 Welch Raod, Suite 154 Palo Alto, California 94304 Phone: (415) 326 - 4248 |

`