CVT GS RAM card jumper settings: (Revision level is on extra leg at bottom)
Rev A: -         Alone     W/Apple card     W/4 meg card
                 A and B
Rev B: - same configuration with or without an Apple Memory card.
1 MB             both under AB
2 MB             #1 under BC, #2 under AB
3 MB             #1 under AB, #2 under AC
4 MB             both under BC

CVT RamFast DIP switches (all are set to off from the factory)
  1. terminator power (on=yes, off=no)  |<| only these two work on
  2. Rom: (off=GS, on=//e)              |<| version 2.0 and above.
  3. Machiene type (off=GS or enhanced //e, on=unenhanced //e)
  4. DMA (off=DMA on)
  5. GS ROM (on=old, off=ROM 03)
  6. RomDisk (off=enable, on=disable)
  7. Drive Search timeout (off=30 seconds, on=3 seconds)
  8. Reserved (must be off)

ZIP GSX Dip Switches:
  SW 1/1 - ON:  cache enable
  SW 1/2 - OFF: enable joystick
  SW 1/3 - ON:  disable AppleTalk Delay
  SW 1/4 - OFF: allows GS self test to pass
  SW 1/5 - OFF: CPS Follow
  SW 1/6 - ON:  enable speed
  SW 1/7 & 1/8 - Cache size: SW 1/7 1/8
                      8K        ON   ON   ZipChipGS
                     16K        ON   OFF  ZipChipGSX, ZipChipGS+
                     32K        OFF  ON
                     64K        OFF  OFF
  SW 2/1 thru SW 2/7 - ON: disable slot delay, (2 is OFF enable delay)
  SW 2/8 - OFF: speaker delay enable

Macintosh Plus, SE SIMM configurations:
 Memory          1st bank  2nd bank         R8/R9 (plus) R35/R36 (SE)
 1 MB            (2) 256K  (2) 256K         R8/xx        R35/xxx
 2 MB            (2) 1024K                  xx/R9        xxx/R36
 2.5 MB          (2) 1024K (2) 256K         xx/xx        xxx/xxx
 4 MB            (2) 1024K (2) 1024K        xx/xx        xxx/xxx

CMS SD 8 DIP switches on back
  1. SCSI ID +4 (when Pressed in on the top)
  2. SCSI ID +2 ( "                      " )
  3. SCSI ID +1 ( "                      " )
  4-7. No connection
  8. Reset (must be pressed in at the top for Apple //'s)

Apple High Speed DMA SCSI Card DIP switches
  1. DMA
  2. \
  3.  | - SCSI ID
  4. /

Laser 128 Bottom config switches (rightmost 2 switches if more than 2)
  Right switch (as seen from bottom)-  Down = enable UDC, up = enable slot 7
  Left switch - Down (twards keyboard) = enable /RAM5,   up = enable slot 5

AE Vulcan DIP switches
  1. Interrupt enable (not used)
  2. GS=closed, //e,][+=open
  3. Boot enable (unenhanced //e,][+=open to boot, otherwise closed)
  4. Pseudo-slot enable (closed=PS slot 7)
      (open=push down on side marked open)

Ram 4000 Jumpers:
  1 Meg: no jumpers
  2 Meg: JP2
  3 Meg: Not supported
  4 Meg: JP1 and JP2

GS ROM 03 internal Jumper S1 disables Control Panel.

Apple Desktop Bus Port pin-outs: (mini-4)
 1 ADB data
 2 NC  Reserved
 3 +5V Power
 4 GND Ground

Apple's GS Memory Expansion Card
  1 Meg: no jumpers
  2 Meg: Jumper on bottom set of prongs
  3 Meg: Not supported
  4 Meg: Both jumpers

Apple Rev 'C' Card:
  Put jumper on ID you want for card: 7 is right-most, 0 is left-most pins.
Only supports Hard Drives and CD-ROM.  Not tape backup, ejectable
media, etc.

Super Writer 924 DIP Switch Functions:
(pressed in at the Top is On=Up, Off=Down)
Mode (Switches 1-2)
 Transparent            Down     Down
 ImageWriter            Down     Up
 ImageWriter II         Up       Down
 ImageWriter LQ         Up       Up
Type (switch 3)
 B/W                    Down
 Color                  Up
Baud (switch 4)
 9600                   Down
 19200                  Up
Printer (switches 5-8)
 Blue Chip              Up       Down    Up      Up
 C-Itoth 8510           
 C-Itoth 8510S          Up       Down    Down    Up
 C-Itoth ProWriter JR+  Down     Down    Up      Up
 Epson MX               Down     Down    Down    Up
 Epson RX               Down     Down    Up      Down
 Epson FX               Down     Down    Up      Up
 Epson JX               Down     Up      Down    Down
 Epson LQ-1500          Down     Up      Down    Up
 IBM Graphics           Down     Up      Up      Down
 NEC 8023               Up       Down    Down    Up
 Okidata 192            Down     Up      Up      Up
 Okidata 292            Up       Down    Down    Down
 ProWriter              Up       Down    Down    Up
 Star (old)             Down     Down    Down    Down
 Star XR-1000/1500      Up       Up      Down    Down
 Star NX-1000           Down     Down    Up      Up
 Star NX-1000R          Down     Up      Down    Down
 Star XB-2410/2415      Down     Up      Down    Up
 Star NB10/15           Down     Up      Down    Up
 Fujitsu DL (color)     Down     Up      Down    Down
 Fujitsu DL B/W         Down     Up      Up      Down
 Fujitsu DX             Down     Down    Up      Up
 Panisonic KXP 1124     Down     Up      Down    Up    (and 1534, 1624)
 Panisonic KXP 1180     Down     Down    Up      Up    (and 1191, 1192)
 Panisonic KXP 1080     Down     Down    Up      Down  (and 1091, 1092)
 24 Pin (mode=LQ)       Down     Up      Down    Up
